head	1.1;
access;
symbols;
locks; strict;
comment	@# @;
expand	@b@;


1.1
date	2002.03.15.00.27.25;	author tri;	state Exp;
branches;
next	;


desc
@@


1.1
log
@Re-Commit documents as binary files.
@
text
@README FILE OF BSQUARE(R) LATE-BREAKING INFORMATION FOR THE General
Election Systems AccuTouch Adaptation


(C) 2001 BSQUARE(R) Corporation - Confidential Data
The information contained herein is intended solely for use 
by BSQUARE Corporation and its licensed customers.  Disclosure, 
reproduction, and any other communication of this material to 
others are strictly prohibited. The subject matter contained 
herein is subject to change.  BSQUARE is a registered trademark 
of BSQUARE Corporation and other marks are the property of the 
respective owners. 

Document No. REL_AccuTouch_1073


________________________
1. Introduction

This document provides late-breaking information
supplementing the documentation for the BSQUARE Global Election 
Systems Adaptation.

________________________
2.  Online Documentation

Information for using the Global Election Systems Adaptation is 
contained in online documentation that can be accessed via your 
desktop. The documentation can be accessed using Adobe Acrobat 
Reader. If you do not have Adobe Acrobat Reader, you can download 
the Reader at:

   http://www.adobe.com

The Global Election Systems User's Manual contains sections with 
sample code.  See the section titled "Copying Sample Code" in the 
introduction of the User's Manual for information on enabling the 
Adobe Reader to select and copy text.

________________________
3.  Touch Screen Limitation

The touch screen does not extend to the outer edges of the screen.  
The user may have difficulty clicking on an item that is on or near 
the edge of the screen.

________________________
4.  Object Store Memory

There is a one-time memory leak of approximately 64K.  This does not
increase over time.

________________________
5.  Audio Driver Limitations

Pitch control and playback rate changes are not supported in the
audio driver at this time.

________________________
6.  Keyboard Issues

The NUMLOCK key is always ON by design.  The F1 function key brings up 
the WindowsCE Start menu.  The CAPSLOCK LED on the key board will not 
light when the CapsLock key is pressed.

________________________
7.  Hardware Keyboard and Soft Input Panel (SIP)

CapsLock on the hardware keyboard and the SIP are not synchronized 
due to a limitation in the MicroSoft SIP code.

________________________
8.  Soft Input Panel - BackQuote key

The 'BackQuote' key on the SIP does not send the right virtual key 
code (sends - 96, expected - 192), due to a limitation in MicroSoft's 
SIP code.

________________________
9.  Flow control on COM4

Hardware flow control is not supported on the COM4 hardware, so the 
user will not be able to use any protocols that require hardware 
flow control.  This includes using the 'remnet' application.

________________________
10.  Parallel downloads

When doing parallel downloads, the printer cable must be disconnected.

________________________
11.  Downloading FLASH bootloader through EPROM

The EPROM loader should only be used to download the FLASH bootloader.  
It is not intended to be used to download a CE image.  Use the FLASH 
bootloader to download the CE image.

________________________
12.  COM4/SmartCard

Because COM4 and SmartCard share the same data lines, only one of the 
two can be in use at any time.











@
